| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
command_data_t Struct Reference

## Public Attributes
uint32_t | bus_id
uint32_t | device_address
uint32_t | endpoint
uint8_t | command
uint32_t | command_frame_number
uint32_t | response_frame_number
uint32_t | command
uint32_t | command_in_frame
uint32_t | response_in_frame
uint32_t | arg0
uint32_t | arg1
uint32_t | data_length
uint32_t | crc32
uint32_t | completed_in_frame
uint32_t | reassemble_data_length
uint8_t * | reassemble_data
uint32_t | reassemble_error_in_frame
union { |
int16_t test_number |
int16_t baudrate |
} | data |

The documentation for this struct was generated from the following files:

- /builds/wireshark/wireshark/epan/dissectors/packet-acr122.c
- /builds/wireshark/wireshark/epan/dissectors/packet-adb.c
- /builds/wireshark/wireshark/epan/dissectors/packet-rfid-pn532.c