| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_tap_iax2_stat_t Struct Reference

## Public Attributes
bool | first_packet
uint32_t | flags
uint16_t | seq_num
uint32_t | timestamp
uint32_t | delta_timestamp
double | bandwidth
iax2_bw_history_item | bw_history [300]
uint16_t | bw_start_index
uint16_t | bw_index
uint32_t | total_bytes
double | delta
double | jitter
double | diff
double | time
double | start_time
double | max_delta
double | max_jitter
double | mean_jitter
uint32_t | max_nr
uint16_t | start_seq_nr
uint16_t | stop_seq_nr
uint32_t | total_nr
uint32_t | sequence
bool | under
int | cycles
uint16_t | pt
int | reg_pt

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-iax2-analysis.h