| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_rtpstream_info_calc Struct Reference

## Public Attributes
char * | src_addr_str
uint16_t | src_port
char * | dst_addr_str
uint16_t | dst_port
uint32_t | ssrc
char * | all_payload_type_names
uint32_t | packet_count
uint32_t | total_nr
uint32_t | packet_expected
int32_t | lost_num
double | lost_perc
double | max_delta
double | min_delta
double | mean_delta
double | min_jitter
double | max_jitter
double | max_skew
double | mean_jitter
bool | problem
double | clock_drift_ms
double | freq_drift_hz
double | freq_drift_perc
double | duration_ms
uint32_t | sequence_err
double | start_time_ms
uint32_t | first_packet_num
uint32_t | last_packet_num

## Member Data Documentation

## ◆ start_time_ms

double _rtpstream_info_calc::start_time_ms

Unit is ms

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/tap-rtp-common.h