| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Here is a list of all documented variables with links to the class documentation for each member:

### - c -

- call_num : _rtpstream_info
- callback : _funnel_packet_menu_t
- callback_data : _funnel_packet_menu_t
- callbacks : _wmem_allocator_t
- callsinfo_hashtable : _voip_calls_tapinfo
- callsinfos : _voip_calls_tapinfo
- can_desegment : _packet_info
- can_expand : wslua_variable_t
- can_tls : tcpcl_peer_t
- can_write_encap : file_type_subtype_info
- cancel_acks : ltp_session_data_t
- cancels : ltp_session_data_t
- cap_end_time : _summary_tally
- cap_len : _frame_data
- cap_pipe_bytes_read : _capture_src
- cap_pipe_bytes_to_read : _capture_src
- cap_pipe_databuf : _capture_src
- cap_pipe_databuf_size : _capture_src
- cap_pipe_fd : _capture_src
- cap_pipe_max_pkt_size : _capture_src
- cap_pipe_modified : _capture_src
- cap_start_time : _summary_tally
- capture_child : capture_options_tag
- capture_filters_list : capture_options_tag
- cb_func : _wtap_module_reg
- cb_name : _wtap_module_reg
- cf_framenr : _ws_info_t
- cfg : _stats_tree
- change_value : decode_as_s
- changed_in_pkn : quic_pp_state
- channel_handles : ssh_peer_data
- channel_info : ssh_peer_data
- chdr_missing : tcpcl_peer_t
- chdr_seen : tcpcl_peer_t
- checkpoints : ltp_session_data_t
- children : _stat_node
- chkp_acks : ltp_session_data_t
- cid : k12_input_info_t
- cinfo : _packet_info
- cipher : SslPacketInfo
- cipher_algo : quic_info_data
- cipher_mode : quic_info_data
- class_meta : _wslua_class
- class_methods : _wslua_class
- cleanup : _wmem_allocator_t, epan_plugin
- client_cids : quic_info_data
- client_dcid_initial : quic_info_data
- client_dcid_set : quic_info_data
- client_grease_quic_bit : quic_info_data
- client_iv : ua_keyset
- client_key : ua_keyset
- client_key_len : ua_keyset
- client_loss_bits_recv : quic_info_data
- client_loss_bits_send : quic_info_data
- client_multipath : quic_info_data
- client_odcid : quic_info_data
- client_retry_processed : quic_info_data
- client_sig_len : ua_keyset
- client_streams : quic_info_data
- clnp_dstref : _packet_info
- clnp_srcref : _packet_info
- closed_msg : capture_options_tag
- code : wtap_bpf_insn_s
- col_buf : col_item_t
- col_custom_dfilter : col_item_t
- col_custom_fields : col_item_t
- col_custom_fields_ids : col_item_t
- col_custom_occurrence : col_item_t
- col_data : col_item_t
- col_expr : col_expr_t, epan_column_info
- col_expr_val : col_expr_t
- col_fence : col_item_t
- col_first : epan_column_info
- col_fmt : col_item_t, epan_app_data_t
- col_last : epan_column_info
- col_title : col_item_t
- color : _wmem_tree_node_t
- color_filter : _frame_data
- columns : epan_column_info
- comId : ComId
- comment : _seq_analysis_item
- comp_gencnt : darwin_md
- compare : _ftype_t
- compat : _c_encoded
- completed : thread_pool
- compress_type : capture_options_tag
- compression_type : _summary_tally, wtap_dumper
- condition : _tvbparse_wanted_t, _wslua_breakpoint_t
- condition_error : _wslua_breakpoint_t
- condition_error_msg : _wslua_breakpoint_t
- conn_addr : media_description_t, session_info_t
- contact_negotiated : tcpcl_conversation_t
- contained_length : tvbuff
- contains : _ftype_t
- content_id : media_content_info_t
- content_len : _SslRecordInfo
- context : _dof_secmode_api_data
- context_id : bpsec_id_t
- contiguous_len : _fragment_head
- control : _tvbparse_wanted_t
- control_port : media_description_t
- control_uri : media_description_t
- conv : edhoc_state_t
- conv_addr_port_endpoints : _packet_info
- conv_array : _conversation_hash_t
- conv_elements : _packet_info
- conv_id : _conversation_item_t
- conv_index : conversation
- conv_num : _seq_analysis_item
- conversation_type_val : conversation_element
- copy_value : _ftype_t
- corr_orig : ltp_tap_info_t
- count : thread_pool
- counter : _stat_node
- counts : _capture_info
- crc_field : bp_block_canonical_t, bp_block_primary_t
- crc_type : bp_block_canonical_t, bp_block_primary_t
- crypto_offset : _quic_crypto_info
- ctype : _conversation_item_t
- cum_bytes : _frame_data
- cur_loc : tcpcl_dissect_ctx_t
- curr_layer_num : _packet_info
- curr_proto_layer_num : _packet_info
- current_namespace : ieee80211_radiotap_iterator
- current_proto : _packet_info
- current_section_number : pcapng_t
- current_stream : _http3_session_info
- currentFile : TrdpXmlContext
- custom_block_data : section_info_t
- custom_cbs : preference